

United 8s - 8 Cylinder Class 2025

The following is a list of rules for the United 8s this class is open to all 8 cylinder only vehicles.

General Rules and Specifications apply Must have a stock appearing body Wheels must fit inside body.

Maximum 10" tires and wheels. No Live telemetry or GPS

No rule on left side or rear percentage. No ride height rule. All cars and drivers must be registered to race.

Must be a 8 cylinder motor

Pump fuel or normal racing fuel only no Alcohol or methanal or exotic fuels. Must have a working transponder to practice or race.

Transponder mounting location is 168 inches, or more, from the front of the front nose of the car to the front of the transponder on the left side of the car.

16.0 seconds. Don't exceed that time. DONT BREAK THE BRACKET TIME SET.